“Bombardier-X” HD –1 Swift Experimental
The professional pilots Pocket Rocket for commuting or ripping around.
For the latest updates on this aircraft, visit www.dickert.ca/swift

Airframe |  |
| Wing Span | 14ft.
| Wing area | 37sq.ft.
| Root Chord | 3.9 ft.
| Dihedral | 2 degree
| Wing Sweep | 45 degree
| Length (less Pitot tube) | 16.3ft
| Height | 6.6ft
| Ground Turning Radius (no braking) |
| Goss Weight | 2500 lb
| Empty Weight | 1500 lb
| Fuel | 825 lb
| Pay Load | 175 lb
| Max Baggage | 25 lb
| Wing Loading | 73.5 lb/sq.ft.
| Stall Warn Speed Clean | 124 KIAS
| Stall Warn Speed Flaps 12 | 104 KIAS
| Stall Warn Speed Flaps 24 | 95 KIAS
| Stall Warn Speed Flaps 38 | 89 KIAS
| Stall Warn Speed Flaps 52 | 84 KIAS
Engine |  |
| Static Trust | 3700lb.
| Reverse trust available |
| Jet inlet area | 3.75 sq. ft.